* Picadae Calibration Programs

sudo dnf install python3-devel jack-audio-connection-kit-devel


prerequisites:
pyyaml
sounddevice
soundfile
pthon-rtmidi

export PYTHONPATH=${HOME}/src/picadae/control/app
python p_ac.py -c p_ac.yml

c 60 60 # caputre note 60 using the full_pulseL[] from the p_ac.yml






# plot third take of note 60 
python plot_seq.py ~/temp/p_ac_3_oa/60 p_ac.yml 3

# record a calibration take: CalibrateKeys.start
uses cfg.full_pulseL[] for the pulse sequence
use cfg.calibrateArgs.holdDutyPctD{} for hold PWM duty cycle

# obsolete plotting function in calibrate_plot.py
python calibrate_plot.py ~/temp/p_ac_3_oa/60/2 p_ac.yml 60






![Plot Seq 1](doc/plot_seq_0.png)

`python plot_seq.py ~/temp/p_ac_3_od/60 p_ac.yml 12`


![Multi Plot 1](doc/multi_plot.svg)

plot_seq.py `do_td_multi_plot(inDir,cfg.analysisArgs,[(36,4), (48,2)] )`

